1. Exit the Vitronics Software.
2. Open Windows Explorer and Browse to the **C:\Program Files\Vitronics\** folder. Make a copy of the **data** folder and paste the entire folder on the desktop. The key files that you will need a copy of are OvenConfiguration.mdb and A32config.mdb. These should be in the **data\db** folder on your desktop. Your recipes and product folders should also be in the **data** folder
3. Start the Vitronics software and login as the System user.
4. Open the **Configure machine** dialog by selecting menu item **Setup->Configure Oven**.
5. Select the proper Machine type from the list and click the **Apply** button.



1. A message stating that this will load Default Configuration settings... Click **Yes** to acknowledge.

 

1. Click the **Exit** button and click **Yes** when prompted to Restart Windows.
2. Click **OK** when prompted that Windows will Restart...
3. The Vitronics Program will shut down but Windows will not automatically Restart.
4. Restart Windows.
5. The Vitronics Software will start with default settings.
6. Once it starts, Exit out of the Vitronics Software.
7. Open the **data/db** folder on your desktop and copy the **a32config.mdb** file.
8. Browse to the **C:\Program Files\Vitronics\Data\db** folder and paste the **a32config.mdb** file.
9. Do the same thing for the **OvenConfiguration.mdb** file. Make sure to copy and paste both files and not drag and drop the files otherwise it will make them read only and you will have other issues.
10. Start the Vitronics Software. The machine should be back to correct configuration and show the correct Series of machine at the top of the Vitronics Software